{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["ESP32_ActuBoard_Contoller_bom"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ESP32_ActuBoard_Contoller_bom","index":0,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Qty","Value","Device","Package","Parts","Description","SPICEPREFIX","MPN"]
[2,null,"PINHD-1X19","1X19","JP102, JP103","PIN HEADER"]
[1,null,"PINHD-1X5","1X05","JP101","PIN HEADER"]
[2,"10uF,10V","C-EUC0805","C0805","C101, C102","CAPACITOR, European symbol","C","LMK212ABJ106KGHT"]
[2,"4.7k","R-EU_R0603","R0603","R101, R102","RESISTOR, European symbol","R","RC0603FR-074K7L"]
[1,"ESP32-ST","ESP32-ST","ESP32-ST","IC101"]