ifconfig:

# ethernet card (modelled by point-to-point link) 0 to router
name: ppp0  inet_addr: 100.1.3.1   MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

name: ppp1  inet_addr: 100.2.3.1   MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

ifconfigend.

route:

100.1.0.0        100.1.3.254      255.255.0.0         G   0   ppp0
100.2.0.0        100.2.3.254      255.255.0.0         G   0   ppp1
routeend.

