ifconfig:

# ethernet card (modelled by point-to-point link) 0 to router
name: ppp0  inet_addr: 10.1.1.1   Mask: 255.255.255.0 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

ifconfigend.

route:

default:        10.1.1.2         0.0.0.0   G   0   ppp0

routeend.

