%description:
Testing Add-IP: Start with a multihomed network. After 10s the server 
asks the client to set the primary address to the second path. 
Retransmissions should then be visible on the second path.
%#--------------------------------------------------------------------------------------------------------------


%#--------------------------------------------------------------------------------------------------------------
%inifile: omnetpp.ini

[General]
network=multihomed
cmdenv-event-banners=false
cmdenv-express-mode = false
tkenv-plugin-path = ../../../etc/plugins
ned-path = .;../../../../src;../../lib

#omnetpp 5.0 - 5.1 compatibility:
eventlog-file = "${resultdir}/${configname}-${runnumber}.elog"
output-scalar-file = "${resultdir}/${configname}-${runnumber}.sca"
output-vector-file = "${resultdir}/${configname}-${runnumber}.vec"
snapshot-file = "${resultdir}/${configname}-${runnumber}.sna"

**.testing = false
**.testTimeout = 0

# udp app (off)
**.numUdpApps = 0
**.udpType = ""

**.numTcpApps = 0
**.tcpType = "TCP"

# sctp apps
**.sctp_client.numSctpApps = 1
**.sctp_client.sctpType="SCTP"
**.sctp_client.sctpApp[0].typename = "SCTPClient"
**.sctp_client.sctpApp[0].localAddress = "10.1.1.1 10.2.1.1 "
**.sctp_client.sctpApp[0].connectAddress = "10.1.3.1"
**.sctp_client.sctpApp[0].primaryPath = "10.1.3.1"
**.sctp_client.sctpApp[0].connectPort = 6666
**.sctp_client.sctpApp[0].requestLength= 1452
**.sctp_client.sctpApp[0].startTime = truncnormal(1s,0.2s)
**.sctp_client.sctpApp[0].stopTime = truncnormal(20s,2s)
**.sctp_client.sctpApp[0].numRequestsPerSession = 100000000
**.sctp_client.sctpApp[0].queueSize = 100
**.sctp_client.sctpApp[0].outboundStreams = 1
**.sctp_client.sctp.chunks = "ASCONF,ASCONF_ACK"
**.sctp_client.sctp.addAddress = ""
**.sctp_client.sctp.addIpType = "0"
**.sctp_client.sctp.addTime = 0s

**.sctp_server.numSctpApps = 1
**.sctp_server.sctpType="SCTP"
**.sctp_server.sctpApp[0].typename = "SCTPServer"
**.sctp_server.sctpApp[*].localAddress = "10.1.3.1 10.2.3.1"
**.sctp_server.sctpApp[0].localPort = 6666
**.sctp_server.sctpApp[*].queueSize = 0 #Size of sendQueue before App is notified to send new data
**.sctp_server.sctpApp[*].numPacketsToSendPerClient = 0
**.sctp_server.sctpApp[*].numPacketsToReceivePerClient = 0
**.sctp_server.sctpApp[*].outboundStreams = 1
**.sctp_server.sctp.chunks = "ASCONF,ASCONF_ACK"
**.sctp_server.sctp.addAddress = "10.2.3.1"
**.sctp_server.sctp.addIpType = "49156" 
#NONE = 0, SET_PRIMARY_ADDRESS= 49156, ADAPTATION_LAYER_INDICATION= 49158, SUPPORTED_EXTENSIONS= 32776,
#ADD_IP_ADDRESS = 49153, DELETE_IP_ADDRESS= 49154, ERROR_CAUSE_INDICATION= 49155, SUCCESS_INDICATION= 49157
**.sctp_server.sctp.addTime = 10s

# sctp settings
**.sctp.sctpAlgorithmClass = "SCTPAlg"
**.sctp.addIP = true



%#--------------------------------------------------------------------------------------------------------------
%contains-regex: results/General-0.sca
scalar multihomed.sctp_client.sctp 	"Number of Fast Retransmissions 1:10.1.3.1" 	[1-9][0-9]*
%#--------------------------------------------------------------------------------------------------------------
