ifconfig:

# ethernet card (modelled by point-to-point link)
name: ppp0  inet_addr: 100.1.1.253 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

# ethernet card (modelled by point-to-point link)
name: ppp1  inet_addr: 100.1.2.253 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

name: ppp2  inet_addr: 100.1.3.254 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST
ifconfigend.

route:
100.1.1.0	100.1.1.254	255.255.255.0		G	0	ppp0
100.1.2.0	100.1.2.254	255.255.255.0		G	0	ppp1
100.1.3.1	100.1.3.1	255.255.255.255 	H 	0	ppp2

routeend.

