ifconfig:

# ethernet card (modelled by point-to-point link)
name: ppp0  inet_addr: 10.2.254.1 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

# ethernet card (modelled by point-to-point link)
name: ppp1  inet_addr: 10.2.254.3 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

# ethernet card (modelled by point-to-point link)
name: ppp2  inet_addr: 10.2.0.2 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST


ifconfigend.

route:
#default:    10.2.0.1    0.0.0.0  G 0 ppp2
10.2.1.0     10.2.254.2        255.255.255.0 G   0   ppp0
10.2.2.0     10.2.254.4        255.255.255.0 G   0   ppp1
#10.1.0.0     10.2.0.1     255.255.0.0  G  0  ppp2
0.0.0.0    10.2.0.1        0.0.0.0   G  0   ppp2

routeend.

