ifconfig:

# ethernet card (modelled by point-to-point link)
name: ppp0  inet_addr: 10.3.254.1 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

# ethernet card (modelled by point-to-point link)
name: ppp1  inet_addr: 10.3.254.3 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

# ethernet card (modelled by point-to-point link)
name: ppp2  inet_addr: 10.3.0.2 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST


ifconfigend.

route:
10.3.1.0     10.3.254.2        255.255.255.0 G   0   ppp0
10.3.2.0     10.3.254.4        255.255.255.0 G   0   ppp1
0.0.0.0    10.3.0.1        0.0.0.0   G  0   ppp2

routeend.
