//
// Copyright (C) 2013 OpenSim Ltd
//
// This program is free software; you can redistribute it and/or
// modify it under the terms of the GNU Lesser General Public License
// as published by the Free Software Foundation; either version 2
// of the License, or (at your option) any later version.
//
// This program is distributed in the hope that it will be useful,
// but WITHOUT ANY WARRANTY; without even the implied warranty of
// MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
// GNU Lesser General Public License for more details.
//
// You should have received a copy of the GNU Lesser General Public License
// along with this program; if not, see <http://www.gnu.org/licenses/>.
//

package inet.physicallayer.apskradio.packetlevel;

import inet.physicallayer.base.packetlevel.NarrowbandReceiverBase;

//
// This receiver model receives a transmission succesfully if the minimum of the
// signal to noise and interference ratio over the duration of the reception is
// sufficiently high. It uses the error model to compute the error rate based on
// this value and the used modulation.
//
// See also ~APSKScalarTransmitter, ~APSKScalarRadio, ~APSKScalarRadioMedium, and
// ~ScalarAnalogModel.
//
module APSKScalarReceiver extends NarrowbandReceiverBase
{
    parameters:
        modulation = default("BPSK");
        errorModelType = default("APSKErrorModel");
        @class(APSKScalarReceiver);
}
