//
// Copyright (C) 2005 Andras Varga
//
// This program is free software; you can redistribute it and/or
// modify it under the terms of the GNU General Public License
// as published by the Free Software Foundation; either version 2
// of the License, or (at your option) any later version.
//
// This program is distributed in the hope that it will be useful,
// but WITHOUT ANY WARRANTY; without even the implied warranty of
// MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
// GNU General Public License for more details.
//
// You should have received a copy of the GNU General Public License
// along with this program; if not, write to the Free Software
// Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA  02111-1307, USA.
//

package inet.examples.wireless.aggregationtest;

import inet.applications.ethernet.EtherAppCli;
import inet.common.queue.Sink;
import inet.linklayer.ieee80211.Ieee80211Nic;
import inet.mobility.static.StationaryMobility;
import inet.networklayer.configurator.ipv4.IPv4NetworkConfigurator;
import inet.node.ethernet.Eth100M;
import inet.node.inet.Router;
import inet.node.inet.StandardHost;
import inet.node.inet.WirelessHost;
import inet.node.wireless.AccessPoint;
import inet.physicallayer.ieee80211.packetlevel.Ieee80211ScalarRadioMedium;


module WirelessAPWithSink
{
    parameters:
        @networkNode();
        @labels(node);
        @display("i=device/accesspoint");
        *.interfaceTableModule = default("");
    gates:
        input radioIn @directIn;
    submodules:
        sink: Sink {
            parameters:
                @display("p=169,124");
        }
        wlan: Ieee80211Nic {
            parameters:
                @display("p=89,225;q=queue");
                mgmtType = default("Ieee80211MgmtAPSimplified");
                mgmt.encapDecap = "false";
        }
        mobility: StationaryMobility {
            parameters:
                @display("p=71,121");
        }
    connections allowunconnected:
        radioIn --> { @display("m=s"); } --> wlan.radioIn;
        wlan.upperLayerOut --> sink.in++;
}

module SinkClient
{
    parameters:
        @display("i=device/wifilaptop");
        @networkNode();
        *.interfaceTableModule = "";
    gates:
        input radioIn @directIn;

    submodules:
        sink: Sink {
            parameters:
                @display("p=65,34");
        }
        wlan: Ieee80211Nic {
            parameters:
                @display("p=112,134;q=queue");
                mgmtType = default("Ieee80211MgmtSTASimplified");
        }
        mobility: StationaryMobility {
            parameters:
                @display("p=50,141");
        }
    connections allowunconnected:
        wlan.radioIn <-- radioIn;
        wlan.upperLayerOut --> sink.in++;
}

module ThroughputClient
{
    parameters:
        @display("i=device/wifilaptop");
        @networkNode();
        *.interfaceTableModule = "";
    gates:
        input radioIn @directIn;
    submodules:
        cli: EtherAppCli {
            parameters:
                registerSAP = false;
                @display("b=40,24;p=180,60,col");
        }
        wlan: Ieee80211Nic {
            parameters:
                @display("p=112,134;q=queue");
                mgmtType = default("Ieee80211MgmtSTASimplified");
        }
        mobility: StationaryMobility {
            parameters:
                @display("p=50,141");
        }
    connections allowunconnected:
        wlan.radioIn <-- radioIn;
        cli.out --> wlan.upperLayerIn;
}

network AggregationTest
{
    parameters:
        int numCli;
        @display("b=297,203");
    submodules:
        cliHost[numCli]: ThroughputClient {
            parameters:
                @display("r=,,#707070");
        }
        ap: WirelessAPWithSink {
            parameters:
                @display("p=200,200;r=,,#707070");
        }
        radioMedium: Ieee80211ScalarRadioMedium {
            parameters:
                @display("p=61,46");
        }
}

network AggregationTest2
{
    @display("bgb=503,221");
    submodules:
        sender1: WirelessHost {
            @display("p=62,35");
        }
        sender2: WirelessHost {
            @display("p=62,117");
        }
        sink1: WirelessHost {
            @display("p=335,130");
        }
        sink2: WirelessHost {
            @display("p=335,35");
        }
        accessPoint: AccessPoint {
            @display("p=205,69");
        }
        configurator: IPv4NetworkConfigurator {
            parameters:
                assignDisjunctSubnetAddresses = false;
                @display("p=455,178");
        }
        radioMedium: Ieee80211ScalarRadioMedium {
            @display("p=62,165");
        }
    connections:
}

