{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["ESP32_ActuBoard_Connector_bom"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ESP32_ActuBoard_Connector_bom","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[null,"ActuBoard Connector A1"]
["Qty","Value","Device","Package","Parts","Description","SPICEPREFIX","MPN"]
[10,"﻿1nF,10V","C-EUC0603","C0603","C202, C203, C204, C205, C206, C301, C302, C303, C304, C305","CAPACITOR, European symbol","C","885012206083"]
[1,null,"PINHD-1X5","1X05","JP101","PIN HEADER"]
[1,null,"PINHD-2X4/90","2X04/90","JP102","PIN HEADER"]
[1,"0R","R-EU_R0603","R0603","R201","RESISTOR, European symbol","R","RC0603FR-070RL"]
[10,"100R","R-EU_R0603","R0603","R202, R203, R204, R214, R215, R301, R302, R303, R313, R314","RESISTOR, European symbol","R","RC0603FR-07100RL"]
[4,"100k","R-EU_R0603","R0603","R101, R102, R103, R104","RESISTOR, European symbol","R","RC0603FR-07100KL"]
[1,"100nF,10V","C-EUC0603","C0603","C102","CAPACITOR, European symbol","C","CC0603MRY5V9BB104"]
[1,"100uF,35V","CPOL-EUE5-8.5","E5-8,5","C201","POLARIZED CAPACITOR, European symbol","C","ESY477M035AH4AA"]
[20,"10k","R-EU_R0603","R0603","R205, R206, R207, R208, R209, R210, R216, R217, R218, R219, R304, R305, R306, R307, R308, R309, R315, R316, R317, R318","RESISTOR, European symbol","R","RC0603FR-0710KL"]
[1,"10uF,10V","C-EUC0805","C0805","C101","CAPACITOR, European symbol","C","LMK212ABJ106KGHT"]
[10,"15EDGRC-3.81-02P-14-00AH","15EDGRC-3.81-02P-14-00AH","15EDGRC-3.81-02P","J202, J203, J204, J205, J206, J301, J302, J303, J304, J305",null,null,"15EDGRC-3.81-02P-14-00AH"]
[10,"20k","R-EU_R0603","R0603","R211, R212, R213, R220, R221, R310, R311, R312, R319, R320","RESISTOR, European symbol","R","RC0603FR-0720KL"]
[1,"2EDGRC-5.08-02P-14-00AH","2EDGRC-5.08-02P-14-00AH","2EDGRC-5.08-02P","J201",null,null,"2EDGRC-5.08-02P-14-00AH"]
[10,"2N7002P","2N7002P","SOT23","Q201, Q202, Q203, Q207, Q208, Q301, Q302, Q303, Q307, Q308",null,null,"2N7002P"]
[10,"CSD17579Q3A","CSD17579Q3A","DNH0008A","Q204, Q205, Q206, Q209, Q210, Q304, Q305, Q306, Q309, Q310","CSD17579Q3A 30V N-Channel NexFET Power MOSFET",null,"CSD17579Q3A"]
[1,"PCA9685PW","PCA9685PW","TSSOP28","IC101","16-channel, 12-bit PWM Fm+ I2C-bus LED controller",null,"PCA9685PW"]
[1,"SMAJ24A","SMAJXXA","DO214AC","D201","SMAJ Transient Voltage Suppressor Diode Series",null,"SMAJ24A"]
[10,"VSSAF5M10","VSSAF5M10","DO-221AC_(SLIMSMA)","D202, D203, D204, D205, D206, D301, D302, D303, D304, D305","Surface Mount Trench MOS Barrier Schottky Rectifier",null,"VSSAF5M10"]