%description:
Testing SCTP congestion control: A multi-homed client sends data to a multi-homed server. 
Due to a lossy link data gets lost and has to be retransmitted. We have to see fast and timer
based retransmissions.   
%#--------------------------------------------------------------------------------------------------------------


%#--------------------------------------------------------------------------------------------------------------
%inifile: omnetpp.ini

[General]
network=multihomed
cmdenv-event-banners=false
cmdenv-express-mode = false
tkenv-plugin-path = ../../../etc/plugins
ned-path = .;../../../../src;../../lib

#omnetpp 5.0 - 5.1 compatibility:
eventlog-file = "${resultdir}/${configname}-${runnumber}.elog"
output-scalar-file = "${resultdir}/${configname}-${runnumber}.sca"
output-vector-file = "${resultdir}/${configname}-${runnumber}.vec"
snapshot-file = "${resultdir}/${configname}-${runnumber}.sna"

**.testing = false
**.testTimeout = 0

# udp app (off)
**.numUdpApps = 0
**.udpType = ""

**.numTcpApps = 0
**.tcpType = "TCP"

# sctp apps
**.sctp_client.numSctpApps = 1
**.sctp_client.sctpType="SCTP"
**.sctp_client.sctpApp[0].typename = "SCTPClient"
**.sctp_client.sctpApp[0].localAddress = "10.1.1.1 10.2.1.1"
**.sctp_client.sctpApp[0].connectAddress = "10.1.3.1"
**.sctp_client.sctpApp[0].primaryPath = "10.1.3.1"
**.sctp_client.sctpApp[0].connectPort = 6666
**.sctp_client.sctpApp[0].requestLength= 1452
**.sctp_client.sctpApp[0].startTime = 1s
**.sctp_client.sctpApp[0].stopTime = 500s
**.sctp_client.sctpApp[0].numRequestsPerSession = 100000000
**.sctp_client.sctpApp[0].queueSize = 100

**.sctp_server.numSctpApps = 1
**.sctp_server.sctpType="SCTP"
**.sctp_server.sctpApp[0].typename = "SCTPServer"
**.sctp_server.sctpApp[0].localAddress = "10.1.3.1 10.2.3.1"
**.sctp_server.sctpApp[0].localPort = 6666
**.sctp_server.sctpApp[*].queueSize = 0 #Size of sendQueue before App is notified to send new data
**.sctp_server.sctpApp[*].numPacketsToSendPerClient = 0
**.sctp_server.sctpApp[*].numPacketsToReceivePerClient = 0

**.finishEndSimulation = true


# sctp settings
**.sctp.sctpAlgorithmClass = "SCTPAlg"



%#--------------------------------------------------------------------------------------------------------------
%contains-regex: stdout
Association 1: number of Fast RTX=[1-9][0-9][0-9]*, number of Timer-Based RTX=[1-9]*
%contains-regex: results/General-0.sca
scalar multihomed.sctp_server.sctp[ \t]*"Number of Bytes received from 3:10.2.1.1"[ \t]*[1-9][0-9]*
%#--------------------------------------------------------------------------------------------------------------
