
# filename: mcrouter1.mrt
# routing table for router 1 of multicast network 2
# connected to host 1,2,3 and router 2
# author: Jochen Reber


ifconfig:

# ethernet card (modelled by point-to-point link)
name: ppp0  inet_addr: 10.1.1.254 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST
name: ppp1  inet_addr: 10.2.1.254 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST
name: ppp2  inet_addr: 10.1.2.253 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST
name: ppp3  inet_addr: 10.2.2.253 MTU: 1500   Metric: 1  POINTTOPOINT MULTICAST

ifconfigend.

route:
10.1.1.1     10.1.1.1        255.255.255.255   H   0   ppp0
10.2.1.1     10.2.1.1        255.255.255.255   H   0   ppp1
10.1.3.0     10.1.2.254      255.255.255.0     G   0   ppp2
10.2.3.0     10.2.2.254      255.255.255.0     G   0   ppp3

routeend.

